For 1990-2009 cars

### Removal Procedure

1. Remove the auto level control air compressor from the vehicle. Refer to Air Compressor Description .
2. Remove the hose from the auto level control air compressor in two places.
3. Remove the auto level control air compressor filter from the hose.

### Installation Procedure

Important: Once you connect the hose to the auto level control air compressor, twist the tie in the hose such that the hose does not contact the rubber shield on the auto level control air compressor.

1. Install the auto level control air compressor filter to the hose.
2. Install the hose to the auto level control air compressor in two places.
3. Install the auto level control air compressor to the vehicle. Refer to Air Compressor Description .