For 1990-2009 cars

### Removal Procedure

1. Remove the loosening screw at the rearview mirror support.
2. Slide the rearview mirror from the rearview mirror support.

### Installation Procedure

1. Locate the rearview mirror support on the windshield.
2. Install the rearview mirror to the rearview mirror support, ensuring that the mirror is fully seated.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screw at the rearview mirror support.

Tighten
Tighten the screws to 2 N·m (18 lb in).