For 1990-2009 cars

### Removal Procedure

1. Remove the auto level control air compressor from the vehicle. Refer to Air Compressor Replacement .
2. Clean the area around the connection of the air dryer (2) to the auto level control air compressor head (1).
3. Rotate the spring clip retaining the dryer to the auto level control air compressor 90 degrees.
4. Remove the air dryer (2) from the air dryer bracket and the auto level control air compressor.

### Installation Procedure

1. Install the air dryer (2) to the air dryer bracket (3) and auto level control air compressor.
2. Rotate the clip 90 degrees in order to retain the dryer to the auto level control air compressor.
3. Install the auto level control air compressor to the vehicle. Refer to Air Compressor Replacement