For 1990-2009 cars

## Generator Rear Brace Replacement 3100 Engine L82

### Removal Procedure

1. Remove the stud from the generator.
2. Remove the nut from the engine stud.
3. Remove the brace.

### Installation Procedure

1. Install the brace to the generator and to the engine stud.
2. Hand tighten the nut and the stud.
3. Install the nut to the engine stud.

Tighten
Tighten the nut to 25 N·m (18 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Make sure that tightening the nut does NOT bind the generator.
5. Install the stud on the generator.

Tighten
Tighten the nut to 25 N·m (18 lb ft).

Make sure that tightening the stud does NOT bind the generator.