For 1990-2009 cars

# Warranty Admin. - May, 1999 Labor Time Guide Update

Subject: | May, 1999 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE |  | J6441 | -- | -- | -- | 0.2 | 0.2 | 0.2 | 0.2
ADD

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

0-.3

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - C/K Platform - New Body Style

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
SEAL, POWER STEERING PUMP SHAFT, OIL - REPLACE |  | E8380 |  |  |  |  |  |  |
V6 |  |  | -- | -- | -- | -- | -- | 0.7 | 0.7
V8 | R |  | -- | -- | -- | -- | -- | 0.9 | 0.9

- PART GP: 6.617

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MIRROR, OUTSIDE REAR VIEW - REPLACE

- No Change to "PART GP," "NOTE," or "INC"

MANUAL |  |  |  |  |  |  |  |  |
RIGHT | R | R3260 | 0.7 | '.7 | 0.7 | 0.7 | 0.7 | 0.7 |
LEFT | N | R3261 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 |
REMOTE CONTROL |  |  |  |  |  |  |  |  |
RIGHT | N | R3280 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 |
LEFT | R | R3281 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 |
ELECTRIC REMOTE CONTROL |  |  |  |  |  |  |  |  |
RIGHT | R | R3290 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.4
LEFT | R | R3291 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.4
ADD: |  |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

- B- To Color/Clear Coat Painted Mirror

R

0.5

GD

0.5

GD

0.5

GD

0.5

GD

0.5

GD

0.5

GD

0.6

GE

*IND: N - New/R - Revised

#### LTG Update - KD/KE Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MOLDING, REAR DOOR - R&R OR REPLACE

- PART GP: 12.114

- INC: R&R or replace fasteners as necessary.

RIGHT |  |  |  |  |  |  |  |  |
SIDE | R | B7966 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.2
LEFT |  |  |  |  |  |  |  |  |
SIDE | R | B7976 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.2
ADD: |  |  |  |  |  |  |  |  |

- A- To Color/Clear Coat

R

--

0.5

GE

0.5

GE

0.5

GE

0.5

GE

0.5

GE

0.4

GD

*IND: N - New/R - Revised

#### LTG Update - Medium Duty Platform

OPERATION | IND* | OP NUM | CAB STYLE YEAR VIN CODE
--- | --- | --- | ---
B | A/W5 | C | H
SENSOR, ENGINE COOLANT TEMPERATURE - REPLACE

- POLICY: E

R

J6368

0.5

--

ST

0.8

ADD: |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

0-.3

--

ST

ST

*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
CORE, HEATER - REPLACE

- PART GP: 8.854

HEATER (NON A/C) | R | D2820 |  |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | -- | -- | 3.3 | 3.3 | 3.3 | 3.3
ACHIEVA & SKYLARK |  |  | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 |  |
GRAND AM & ALERO |  |  | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 | 1.1 | 1.1
A/C | R | D2822 |  |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | -- | -- | 3.3 | 3.3 | 3.3 | 3.3
ACHIEVA & SKYLARK |  |  | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 |  |
GRAND AM & ALERO |  |  | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 | 1.1 | 1.1
AMPLIFIER, RADIO - REPLACE | N | R0820 | -- | -- | -- | -- | -- | 0.2 | 0.2
ADD: |  |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MODULE, WINDSHIELD WIPER - REPLACE | N | N3565 | -- | -- | -- | 0.5 | 0.5 | 0.5 | 0.5
ADD: |  |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

0-.3

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
REGULATOR, REAR DOOR WINDOW - R&R OR REPLACE

- No Change to "PART GP," "INCs," or "NOTE"

RIGHT MANUAL |  | C0380 | 0.6 | 0.6 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
LEFT MANUAL |  | C0381 | 0.6 | 0.6 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
RIGHT POWER |  | C0382 |  |  |  |  |  |  |
CHEVROLET |  |  | 0.8 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
PONTIAC |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
OLDSMOBILE |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.6 | 0.6 | 0.6
BUICK |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
LEFT POWER |  | C0383 |  |  |  |  |  |  |
CHEVROLET |  |  | 0.8 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
PONTIAC |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
OLDSMOBILE |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.6 | 0.6 | 0.6
BUICK |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
ADD: |  |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

R

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

CYLINDER, IGNITION LOCK - R&R OR REPLACE

- PART GP: 2.188

- INC: Disable and Enable SIR System

R

E7200

CHEVROLET |  |  | 1.5 | 1.5 | 1.5 | 1.4 | 1.4 | 1.4 | 1.4
PONTIAC |  |  | 1.5 | 1.5 | 1.5 | 0.5 | 0.5 | 0.5 | 0.5
OLDSMOBILE |  |  | 1.5 | 1.5 | 1.5 | 1.5 | 1.1 | 1.1 | 1.1
BUICK |  |  | 1.5 | 1.5 | 1.5 | 0.6 | 0.6 | 0.6 | 0.6
ADD: |  |  |  |  |  |  |  |  |

- A- To Code Cyl

--

--

--

0.3

0.3

0.3

0.3

- B- For Cylinders That Will Not Rotate

- Pontiac/Buick

R

--

--

--

1.0

1.0

1.0

1.0

*IND: N - New/R - Revised