For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Do the high beam headlamps turn ON? | -- | Go to Step 2 | Go to Headlight System Check
2 | Do the turn signal indicators work when the turn signals are on? | -- | Go to Step 3 | Go to Instrument Cluster Illumination Lamps Inoperative
3 | Test for a poor connection or an open in circuit 11 between the instrument cluster harness connector C2 terminal Q and S219. Did you find a poor connection or an open? | -- | Go to Step 4 | Go to Step 5
4 | Repair the poor connection or an open in circuit 11 between the instrument cluster harness connector C2 terminal Q and S219. Has the repair been made and the system rechecked? | -- | System OK | --
5 |

1. Test the high beam indicator bulb and the bulb connection.
2. If OK, replace the instrument cluster. Refer to Instrument Cluster Replacement .

Has the repair been made and the system rechecked?

--

System OK

--