For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Brake Modulator Bleeder Valves | 9 N·m | 80 lb in
Bleeder Valve (Front Caliper) | 13 N·m | 115 lb in
Bleeder Valve (Rear Wheel Cylinder) | 7 N·m | 62 lb in
Brake Booster Mounting Nuts * | 25 N·m | 18 lb ft
Brake Hose Bolt | 44 N·m | 33 lb in
Brake Pedal Brace to Bracket Nuts | 10 N·m | 89 lb in
Brake Pedal Brace Upper Bolt | 10 N·m | 89 lb in
Brake Pedal Bracket Mounting Nuts | 25 N·m | 18 lb ft
Brake Pipe Fitting Connections (All) | 21 N·m | 15 lb ft
Proportioning Valve Caps | 27 N·m | 20 lb ft
Traction Control Module Bleeder Valves | 9 N·m | 80 lb in
Traction Control Module Bolt to Bracket | 5 N·m | 44 lb in
Tube Nut to Modulator | 24 N·m | 18 lb ft
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating.

| Refer to the appropriate service procedure for the prevailing torque value.

If the fastener does not meet these criteria, REPLACE the fastener.