For 1990-2009 cars

### Removal Procedure

1. Remove the generator front brace if it is a Valeo generator.
2. Remove the generator rear brace nut and bolt.
3. Remove the generator rear brace from the engine.

### Installation Procedure

1. Install the generator rear brace to the engine.
2. Install the generator rear brace nut and bolt.

Tighten
Tighten the generator front brace nut to 25 N·m (18 lb ft).

Tighten
Tighten the generator front brace bolt to 25 N·m (18 lb ft).

3. Install generator front brace if it is a Valeo generator.