For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Remove the sliding door garnish molding. Refer to Rear Side Door Garnish Molding Replacement .
2. Remove the sliding door inside handle. Refer to Sliding Door Inside Handle Replacement .
3. Use the J 38778 in order to remove the sliding door inner trim panel fasteners.
4. Remove the sliding door inner trim panel from the sliding door.

### Installation Procedure

1. Position the sliding door inner trim panel to the sliding door.
2. Align the locating pins on the sliding door inner trim panel to the sliding door.
3. Firmly press the sliding door inner trim panel with the retainers to the sliding door to the seat retainers.
4. Install the sliding door inside handle. Refer to Sliding Door Inside Handle Replacement .
5. Install the sliding door garnish molding. Refer to Rear Side Door Garnish Molding Replacement .