For 1990-2009 cars

Condition | Action
--- | ---
The power steering fluid is low. | Fill the power steering system. Refer to Refilling the Power Steering System .
The power steering fluid is too thick (ambient temperature is -12°C (10°F) or lower). |

• | Drain the power steering system. Refer to Draining the Power Steering System .

• | Fill the power steering system with cold climate fluid. Refer to Fluid and Lubricant Recommendations in Maintenance and Lubrication and Refilling the Power Steering System .

The power steering pump pressure is too low. |

• | Inspect the pump pressure. Refer to Power Steering Gear and Pump Leaks .

• | Repair the pump, as needed. Refer to Power Steering Pump Replacement .

The steering gear is binding. | Repair or replace the power steering gear as necessary. Refer to Steering Gear Replacement .
The steering intermediate shaft is not installed properly. | Repair or replace the intermediate shaft seal as necessary.
The intermediate shaft bolt torque is too high. | Install the intermediate shaft bolt to specification. Refer to Lower/Upper Intermediate Steering Shaft Replacement in Steering Wheel and Column.
The power steering pump or the power steering gear has an internal leak. | Repair or replace the appropriate component as necessary. Refer to Power Steering Pump Replacement or Steering Gear Replacement .
The steering gear valve is sticking. |

1. Drain the power steering system. Refer to Draining the Power Steering System .
2. Fill the power steering system. Refer to Refilling the Power Steering System .
3. Bleed the power steering system. Refer to Power Steering System Bleeding .
4. Repair or replace the power steering gear if the symptoms persist. Refer to Steering Gear Replacement .