For 1990-2009 cars

Application | Service Allowed (Acceptable) | Service Preferred (Target)
--- | --- | ---
Front

- Camber

-1.20 to -0.20 degrees

-0.70 degrees

- Caster (Nominal - No Means of Adjustment Provided)

2.40 to 3.40 degrees

2.90 degrees

- Cross Camber

-0.75 to 0.75 degrees

0 degrees

- Cross Caster (Nominal - No Means of Adjustment Provided)

-0.75 to 0.75 degrees

0 degrees

- Total Toe

-0.20 to 0.20 degrees

0 degrees

Rear (Nominal - No Means of Adjustment Provided)

- Camber

-0.75 to -1.25 degrees

-1.0 degrees

- Cross Camber

-0.50 to 0.50 degrees

0 degrees

- Total Toe

-0.30 to 0.30 degrees

0 degrees