For 1990-2009 cars

### Removal Procedure

1. Remove the driver's side instrument panel insulator retainers.
2. Remove the driver's side instrument panel insulator.
3. Cut the plastic tie strap securing the video entertainment system relay to the wire harness.
4. Disconnect the video entertainment system relay electrical connector.
5. Remove the video entertainment system relay from the vehicle.

### Installation Procedure

1. Install the video entertainment system relay to the vehicle.
2. Connect the video entertainment system electrical connector.
3. Secure the video entertainment system to the wire harness with a plastic tie strap.
4. Install the driver's side instrument panel insulator.
5. Install the driver's side instrument panel retainers.