For 1990-2009 cars

### Removal Procedure

1. Remove the cable from the throttle lever and accelerator control cable bracket.
2. Rotate the cable counter clockwise at the module in order to remove the cable from the module.
3. Remove the cable from the module band.

### Installation Procedure

Important: Ensure that the module strap is not twisted during the installation of the cable.

1. Install the cable to the module band.
2. Install the cable to the module.
3. Install the cable to the throttle lever and accelerator control cable bracket.
4. Adjust the cruise control cable. Refer to Cruise Control Cable Adjustment .