For 1990-2009 cars

### Removal Procedure

1. Fold the cup holder to the open position.
2. Remove the cup holder screws.
3. Remove the cup holder.

### Installation Procedure

1. Install the cup holder.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the cup holder screws.

Tighten
Tighten the cup holder screws to 9 N·m (80 lb in).

3. Fold the cup holder to the closed position.