For 1990-2009 cars

# Power Sliding Door Edge Guard Comes Loose (Install New Edge Guard)

Subject: | Power Sliding Side Door Edge Guard Comes Loose (Install New Edge Guard)

Models: | 1997-2000 Chevrolet Venture

| 1997-2000 Oldsmobile Silhouette

| 1997-1999 Pontiac Trans Sport

| 1999-2000 Pontiac Montana

This bulletin is being revised to update parts information. Please discard Corporate Bulletin Number 00-08-64-015 (Section 08 -- Body & Accessories).

### Condition

Some customers may comment that the door edge guard has started to come off or the over-slam bumper has fallen off.

### Cause

A loss of adhesion to the body may have occurred.

### Correction

1. If the over-slam bumper is missing, clean the surface of the door and install the bumper just below the body feature line (see Figure).
2. Install the new door edge guard just below the over-slam bumper. The new door edge guard pushes over the hem flange on the front leading edge of the door (see Figure).

### Parts Information

Part Number | Description
--- | ---
10301715 | Guard Rear, Side Door Edge
10298620 | Bumper, Rear Side Door RR Upper

Parts are currently available from GMSPO.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C1635 | Guard, Sliding Door Edge - Replace | 0.2 hr