For 1990-2009 cars

### Removal Procedure

1. Remove the HEADLAMP circuit breaker.
2. Remove the inflatable restraint steering wheel module. Refer to Steering Wheel Inflator Module Replacement .
3. Remove the steering wheel. Refer to Steering Wheel Replacement .
4. Remove the steering column shrouds. Refer to Steering Column Shrouds - Disassemble.
5. Disconnect the steering column electrical connectors.
6. Remove the turn signal multifunction switch connectors from the steering column electrical connector.
7. Remove the turn signal multifunction switch. Refer to Turn Signal and Multifcn Sw Assembly - Disassemble.

### Installation Procedure

1. Install the turn signal multifunction switch. Refer to Turn Signal and Multifunction Switch Assembly - Assemble.
2. Install the turn signal multifunction switch connectors to the steering column electrical connector.
3. Connect the steering column electrical connectors.
4. Install the steering column shrouds. Refer to Steering Column Shrouds - Assemble.
5. Install the steering wheel. Refer to Steering Wheel Replacement .
6. Install the inflatable restraint steering wheel module. Refer to Steering Wheel Inflator Module Replacement .
7. Install the HEADLAMP circuit breaker.