For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Carefully peel off the water deflector.

### Installation Procedure

Important: Proper adhesive bonding of the front door water deflector to the inner panel is critical in order to prevent water leaks.

1. Roll the water deflector onto the door panel.
2. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .