For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the exhaust system muffler. Refer to Muffler Replacement .
3. Use a drill in order to remove the rivets at the exhaust muffler heat shield.
4. Remove the exhaust muffler heat shield from the vehicle.

### Installation Procedure

1. Install the exhaust muffler heat shield to the vehicle with new rivets.
2. Install the exhaust system muffler. Refer to Muffler Replacement .
3. Lower the vehicle.