For 1990-2009 cars

Incandescent lamps provide instrument cluster lighting for the following components:

• | The speedometer

• | The tachometer

• | The voltmeter

• | Oil pressure indicator

• | Fuel level indicator

• | The temperature gauges

• | The turn signals indicator

• | The high-beam indicator

• | The liftgate ajar indicator

• | The sliding door ajar indicator

• | The parking brakes indicator

• | The brake fluid level indicator

• | The seat belts indicator

• | The malfunction indicator lamp (MIL) indicator

• | The antilock brakes indicator

• | The traction control indicator

• | The air bag (SIR) indicator

• | The PASS-Key indicator

All of these incandescent lamps are accessible from the back of the instrument cluster. If you need to replace a bulb, removal of the instrument cluster is required. For instrument cluster removal procedures, refer to Instrument Cluster Replacement .