For 1990-2009 cars

# Warranty Administation - August, 2000 Labor Time Guide Updates

Subject: | Warranty Administration -- August, 2000 Labor Time Guide Updates

Models: | 1996-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

#### LTG Update - All Applicable Platforms

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
A/C SYSTEM - LEAK TEST DISCHARGED SYSTEM

- NOTE: This diagnosis time is to be used when necessary to re-charge the A/C system and locate a leak with an electronic leak detector and/or flourescent dye.

N

0.1-0.5

0.1-0.5

0.1-0.5

0.1-0.5

0.1-0.5

0.1-0.5

- NOTE: This labor operation is for reference only. The actual time to perform the diagnosis should be included in "Regular Labor Hours" for the repair of the labor operation submitted.

- NOTE: If leak can not be found, use labor operation D4450.

A/C SYSTEM - LEAK TEST DYE DIAGNOSIS

- NOTE: This labor operation is to to be used when necessary to re-charge the A/C system and add flourescent dye. This labor operation was created in the event that a leak could not be found and the customer would bring the vehicle back at a later date.

N

D4450

0.1-0.5

0.1-0.5

0.1-0.5

0.1-0.5

0.1-0.5

0.1-0.5

- NOTE: Only the system capacity of R134a refrigerant and one bottle flourescent dye can be charged to the warranty repair order.

*IND: N - New/R - Revised

#### LTG Update - C Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.3

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE

- PART GP: 3.130

- POLICY: E

J6391

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

VALVE, EVAPORATIVE EMISSION CANISTER PURGE VACUUM - REPLACE |  | J6441 | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ARM, PITMAN - REPLACE

- PART GP: 6.859

- NOTE: For check and adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

- THE PREVIOUS "NOTE" NO LONGER APPLIES TO LABOR OPERATION E7900.

R

E7900

C TRUCK |  |  | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
K TRUCK |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 |
ADD: |  |  |  |  |  |  |  |

- A- W/Hydraulic Brake Booster

0.1

0.1

0.1

0.1

0.1

0.1

BEARING, CRANKSHAFT MAIN - REPLACE

- PART GP: 0.096

J1150

- INC: Use of plastic type gauge

- NOTE: Applies to V8 Engine, Codes H, K, M, R

ONE BEARING |  |  |  |  |  |  |  |
MANUAL TRANS | R |  |  |  |  |  |  |
C TRUCK |  |  | 6.8 | 6.8 | 6.8 | 6.8 | 6.8 |
K TRUCK |  |  | 6.8 | 6.8 | 6.8 | 6.8 | 6.8 |
AUTO TRANS | R |  |  |  |  |  |  |
C TRUCK |  |  | 6.8 | 6.8 | 6.8 | 6.8 | 6.8 |
K TRUCK |  |  | 6.8 | 6.8 | 6.8 | 6.8 | 6.8 |
3500 HD | R |  |  |  |  |  |  |
AUTO TRANS |  |  | 4.6 | 4.6 | 4.6 | 4.6 | 4.6 | 4.6
MANUAL TRANS |  |  | 3.8 | 3.8 | 3.8 | 3.8 | 3.8 | 3.8
ADD: |  |  |  |  |  |  |  |

- A- W/Engine Oil Cooler

0.1

0.1

0.1

0.1

0.1

0.1

- B- W/Skid Plate

0.2

0.2

0.2

0.2

0.2

- C- To Replace Main Bearings (Each Additional)

R

0.2

0.2

0.2

0.2

0.2

0.2

- D- To Replace All Main Bearings

R

0.7

0.7

0.7

0.7

0.7

0.7

- E- To Replace Connecting Rod Bearings (Each)

R

0.2

0.2

0.2

0.2

0.2

0.2

- F- To Replace All Connecting Rod Bearings

R

1.3

1.3

1.3

1.3

1.3

1.3

- G- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers if Nec

0.2

0.2

0.2

0.2

0.2

0.2

CRANKSHAFT - REPLACE

- NOTE: Applies to V8 Engine, Codes H, K, M, R

J1200

- No Change to "INC" or "PART GP"

C TRUCK | R |  | 7.3 | 7.3 | 7.3 | 7.3 | 7.3 |
K TRUCK | R |  | 7.3 | 7.3 | 7.3 | 7.3 | 7.3 |
3500 HD |  |  | 7.7 | 7.7 | 7.7 | 7.7 | 7.7 | 7.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C

0.6

0.6

0.6

0.6

0.6

0.6

- B- With A.I.R.

R

0.1

0.1

0.1

0.1

0.1

0.1

- C- W/Engine Oil Cooler

0.3

0.3

0.3

0.3

0.3

0.3

- D- To R&R Cyl Head

One |  |  | 1.5 | 1.5 | 1.5 | 1.5 | 1.5 | 1.5
Both |  |  | 1.8 | 1.8 | 1.8 | 1.8 | 1.8 | 1.8

- E- To Replace Piston Rings Only (INC: Ream ridge, check all ring clearances and clean grooves as nec).

Each Piston |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
All Pistons |  |  | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 | 1.6
F- To Replace Rod Only (INC: Ream ridge). |  |  |  |  |  |  |  |
Each Rod |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
All Rods |  |  | 3.7 | 3.7 | 3.7 | 3.7 | 3.7 | 3.7
G- To Replace Piston (INC: Ream ridge and R&R rod from piston. Check piston for size and wear. Check bore size, taper, and out of round. Check piston fit and all ring clearances). |  |  |  |  |  |  |  |
Each Piston |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
All Pistons |  |  | 3.7 | 3.7 | 3.7 | 3.7 | 3.7 | 3.7
H- To Clean Part On Vehicles Over 30,000 Miles/48,000 Kilometers if Nec |  |  | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
CRANKSHAFT - REPLACE

- NOTE: Applies to V8 Diesel Engine, Codes F, P, S

- No Change to "INC", "PART GP" or "POLICIES"

J1200

LEFT HAND DRIVE |  |  | 12.9 | 12.9 | 12.9 | 12.9 | 12.9 | 12.9
RIGHT HAND DRIVE | R |  | -- | -- | 11.7 | 11.7 | 11.7 |

- No Change to "ADD" Conditions

RADIATOR ASSEMBLY - R&R

- NOTE: No Change to "PART GP", "POLICY", "INC" or "NOTE"

J3080

GAS | R |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
DIESEL |  |  | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9

- NOTE: No Change to "ADD" Conditions

*IND: N - New/R - Revised

#### LTG Update - C/K - New Body Style - Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE

- POLICY: E

J6391

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE | N | J6441 | -- | -- | -- | 0.3 | 0.3 | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - E Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.2

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

COMPRESSOR ASSEMBLY - REPLACE

- PART GP: 9.170

D4440

1.2

1.2

1.2

1.2

1.2

1.2

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

0.5

0.5

0.5

0.5

0.5

- B- To Install Liquid Line Filter (THIS "ADD" CONDITION HAS BEEN DELETED)

R

*IND: N - New/R - Revised

#### LTG Update - E/J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
NET, REAR COMPONENT CARGO - REPLACE | N | C4610 |  |  |  |  | 0.2 | 0.2
VALVE, EVPORATIVE EMISSION CANISTER CONTROL - REPLACE |  | J6324 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
*IND: N - New/R - Revised

#### LTG Update - F Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE - REPLACE | N | D3255 |  |  |  |  |  | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.3

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

PUMP, ENGINE OIL - REPLACE

- PART GP: 1.652

- NOTE: Applies to V8 Engine, Code G and P

- No Change to "ADD" Condition

J1020

- MANUAL TRANS

R

3.8

3.8

5.8

5.8

5.4

5.4

- AUTO TRANS

2.2

2.2

4.5

4.5

4.5

4.5

SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
VALVE, EVAPORATIVE EMISSION CANISTER PURGE VACUUM - REPLACE |  | J6441 | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.3

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

*IND: N - New/R - Revised

#### LTG Update - G Van Platform

OPERATION DESCRIPTIO | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
RESISTOR, BLOWER MOTOR - REPLACE

- PART GP: 9.275

- NOTE: No Change to Labor Operations D1000, D1001 or D1005

R

D1002

A/C GAS |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
A/C DIESEL |  |  | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4

- No Change to "ADD" Conditions

FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.4
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System Without C69, Rear Auxiliary A/C

0.5

- B- Recover/Recharge A/C System With C69, Rear Auxiliary A/C

0.7

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.8

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System Without C69, Rear Auxiliary A/C

0.5

- B- Recover/Recharge A/C System With C69, Rear Auxiliary A/C

0.7

PISTON, ROD AND/OR RINGS - REPLACE

- PART GP: 0.626

- No Changes to "INCs"

- NOTE: No Change to Labor Operations J1300 or J1301

- NOTE: Applies to V8 Engine, Code R

BOTH BANKS | R | J1307 | 12.4 | 12.4 | 12.4 | 12.4 | 12.4 | 12.4
ADD: |  |  |  |  |  |  |  |

- A- With A/C

0.7

- B- With Rear A/C

N

0.8

0.8

0.8

0.8

0.8

0.8

- C- W/Cruise Control

0.3

0.3

0.3

0.3

0.3

0.3

- D- W/Engine Oil Cooler

N

0.1

0.1

0.1

0.1

0.1

0.1

- E- To Recondition All Valves

- One Bank

N

1.4

1.4

1.4

1.4

1.4

1.4

- Both Banks

N

2.8

2.8

2.8

2.8

2.8

2.8

- F- To Replace Rings Only

- Each Additional Piston

R

0.2

0.2

0.2

0.2

0.2

0.2

- All Pistons

R

1.3

1.3

1.3

1.3

1.3

1.3

- G- To Replace Rod Only

- Each Additional Rod

0.5

0.5

0.5

0.5

0.5

0.5

- All Rods

R

3.1

3.1

3.1

3.1

3.1

3.1

- H- To Replace Piston

- Each Additional Piston

0.5

0.5

0.5

0.5

0.5

0.5

- All Pistons

R

2.8

2.8

2.8

2.8

2.8

2.8

- I- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec

- Right or Left

0.3

0.3

0.3

0.3

0.3

0.3

- Both

0.4

0.4

0.4

0.4

0.4

0.4

VENT, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6389 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.3

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE

- PART GP 3:130

- POLICY: E

J6391

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PANEL/CARRIER ASSEMBLY, INSTRUMENT CONTROL - REPLACE

- NOTE: No Change to "PART GP", or "INCs"

C2540

CHEVROLET | R |  | 1.9 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9
PONTIAC |  |  | 2.2 | 2.2 | 2.2 | 2.2 | 2.2 | 2.2

- No Change to "ADD" Conditions

FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.8

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6441 | 0.2 | 0.2 | 0.3 | 0.3 | 0.3 | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

SWITCH ASSEMBLY, AUTO TRANS FLUID PRESSURE - REPLACE | R | K6351 | 6.3 | 6.3 | 6.3 | 6.3 | 6.3 | 6.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

- NOTE: No Change to Remaining "ADD" Conditions.

SHAFT AND/OR SEAL, MANUAL - REPLACE |  |  |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours.

R

SHAFT |  | K6501 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 | R |  | -- | -- | -- | 8.6 | 8.6 | 8.6
SEAL |  | K6529 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 | R |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- B- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

LEVER, DETENT - REPLACE |  | K6502 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours.

R

ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 | R |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

WIRING HARNESS AND/OR SOLENOID - REPLACE

- POLICY: E

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours.

R

1 - 2 SHIFT SOLENOID |  | K6555 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 6.2 | 6.2 | 6.2 | 6.2 | 6.2 | 6.2
ENGINE CODE 4 | R |  | -- | -- | -- | 6.7 | 6.7 | 6.7
2 - 3 SHIFT SOLENOID |  | K6556 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 6.2 | 6.2 | 6.2 | 6.2 | 6.2 | 6.2
ENGINE CODE 4 | R |  | -- | -- | -- | 6.7 | 6.7 | 6.7
TCC PWM SOLENOID |  | K6557 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 6.2 | 6.2 | 6.2 | 6.2 | 6.2 | 6.2
ENGINE CODE 4 | R |  | -- | -- | -- | 6.7 | 6.7 | 6.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SLEEVE, OUTPUT SHAFT (LEFT) - REPLACE |  | K6942 | 6.2 | 6.2 | 6.2 | 6.2 | 6.2 | 6.2

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

TRANSAXLE ASSEMBLY - REPLACE

- PART GP: 4.003

K7000

- INC: Cooler line flush, transfer parts, perform Fluid Checking and Functional Test procedures (as outlined in the service manual), and packaging time for Service Replacement Transmission Assembly (SRTA).

R

- NOTE: This operation is for transmission/transaxle replacement only. For transmission/transaxle R&R times use operation J1400.

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours.

R

ENGINE CODES D & T |  |  |  |  |  |  |  |
ENGINE CODE 4 | R |  | -- | -- | -- | 6.2 | 6.2 | 6.2

- NOTE: Disassemble, inspect and reassemble add time to be used as needed when it has been determined that the cost of overhaul exceeds the cost of replacement.

ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CONVERTER ASSEMBLY, TRANSAXLE - REPLACE

- PART GP: 4.115

K7020

- INC: Cooler line flush, oil pressure test, clean and inspect parts and all necessary measurements and adjustments.

R

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 7.1 | 7.1 | 7.1 | 7.1 | 7.1 | 7.1
ENGINE CODE 4 | R |  | -- | -- | -- | 6.2 | 6.2 | 6.2
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SEAL, TRANSAXLE CONVERTER - REPLACE

- PART GP: 4.226

K7060

- NOTE: Does not include oil cooler line flush or diagnosis time.

N

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

ENGINE CODES D & T |  |  | 7.2 | 7.2 | 7.2 | 7.2 | 7.2 | 7.2
ENGINE CODE 4 | R |  | -- | -- | -- | 5.0 | 5.0 | 5.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

PUMP, TRANSAXLE OIL - R&R OR REPLACE |  | K7121 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.2 | 8.2 | 8.2 | 8.2 | 8.2 | 8.2
ENGINE CODE 4 | R |  | -- | -- | -- | 7.2 | 7.2 | 7.2
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

VALVE ASSEMBLY, CONTROL AND GASKET - REPLACE |  | K7123 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.6 | 8.6 | 8.6 | 8.6 | 8.6 | 8.6
ENGINE CODE 4 | R |  | -- | -- | -- | 7.7 | 7.7 | 7.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SPACER PLATE, CHECK BALL AND GASKET - REPLACE |  | K7128 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.6 | 8.6 | 8.6 | 8.6 | 8.6 | 8.6
ENGINE CODE 4 | R |  | -- | -- | -- | 7.7 | 7.7 | 7.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SPACER PLATE, CHECK BALL AND GASKET - REPLACE |  | K7221 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.6 | 9.6 | 9.6 | 9.6 | 9.6 | 9.6
ENGINE CODE 4 | R |  | -- | -- | -- | 8.7 | 8.7 | 8.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SHAFT, TURBINE - REPLACE |  | K7222 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

O-RING, TURBINE SHAFT- REPLACE |  | K7224 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 6.9 | 6.9 | 6.9 | 6.9 | 6.9 | 6.9
ENGINE CODE 4 | R |  | -- | -- | -- | 6.0 | 6.0 | 6.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SHAFT, PUMP DRIVE - REPLACE |  | K7226 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.1 | 8.1 | 8.1 | 8.1 | 8.1 | 8.1
ENGINE CODE 4 | R |  | -- | -- | -- | 7.2 | 7.2 | 7.2
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SHAFT, OUTPUT - R&R OR REPLACE |  | K7325 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 9.6 | 9.6 | 9.6 | 9.6 | 9.6 | 9.6
ENGINE CODE 4 | R |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CHANNEL PLATE AND/OR GASKET - REPLACE |  |  |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

PLATE |  | K7461 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
GASKET |  | K7462 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

ACCUMULATOR, 1-2; PISTON, SEAL OR SPRING - REPLACE |  | K7465 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

ACCUMULATOR, 2-3; PISTON, SEAL OR SPRING - REPLACE |  | K7466 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

ACCUMULATOR, 3-4; PISTON, SEAL OR SPRING - REPLACE |  | K7467 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SPROCKET, DRIVE - REPLACE |  | K7504 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.9 | 8.9 | 8.9 | 8.9 | 8.9 | 8.9
ENGINE CODE 4 | R |  | -- | -- | -- | 8.0 | 8.0 | 8.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SPROCKET, DRIVEN - REPLACE |  | K7506 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 8.8 | 8.8 | 8.8 | 8.8 | 8.8 | 8.8
ENGINE CODE 4 | R |  | -- | -- | -- | 7.9 | 7.9 | 7.9
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

LINK ASSEMBLY, TRANSAXLE DRIVE - REPLACE

- PART GP: 4.131

K7520

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

R

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

ENGINE CODES D & T |  |  | 8.8 | 8.8 | 8.8 | 8.8 | 8.8 | 8.8
ENGINE CODE 4 | R |  | -- | -- | -- | 7.9 | 7.9 | 7.9
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SUPPORT AND SEALS, DRIVE SPROCKET - REPLACE |  | K7522 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.6 | 9.6 | 9.6 | 9.6 | 9.6 | 9.6
ENGINE CODE 4 | R |  | -- | -- | -- | 8.7 | 8.7 | 8.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SENSOR, INPUT SPEED - REPLACE |  | K7524 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 7.6 | 7.6 | 7.6 | 7.6 | 7.6 | 7.6
ENGINE CODE 4 | R |  | -- | -- | -- | 6.7 | 6.7 | 6.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

HARNESS ASSEMBLY, CONTROL WIRE - REPLACE |  | K7526 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 7.7 | 7.7 | 7.7 | 7.7 | 7.7 | 7.7
ENGINE CODE 4 | R |  | -- | -- | -- | 6.8 | 6.8 | 6.8
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SUPPORT, DRIVEN SPROCKET - REPLACE |  | K7529 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

R

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

ENGINE CODES D & T |  |  | 9.2 | 9.2 | 9.2 | 9.2 | 9.2 | 9.2
ENGINE CODE 4 | R |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CLUTCH, SECOND - R&R OR REPLACE |  | K7531 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.2 | 9.2 | 9.2 | 9.2 | 9.2 | 9.2
ENGINE CODE 4 | R |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SPRAG ASSEMBLY, INPUT - REPLACE |  | K7537 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.8 | 9.8 | 9.8 | 9.8 | 9.8 | 9.8
ENGINE CODE 4 | R |  | -- | -- | -- | 8.9 | 8.9 | 8.9
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

ACTUATOR ASSEMBLY, PARK LOCK - REPLACE |  |  |  |  |  |  |  |

- ATTENTION: The following "INC" has been deleted from this labor operation.

- INC: Cooler line flush, oil pressure test, setting T.V. cable, clean and inspect parts and all necessary measurements and adjustments.

R

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

- NOTE: Select the Operation that best describes the primary cause of failure.

PARKING LOCK ACTUATOR |  | K7541 |  |  |  |  |  |
ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 | R |  | -- | -- | -- | 7.9 | 7.9 | 7.9
ADD: |  |  |  |  |  |  |  |

- E- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

GUIDE AND SEAL, PARK LOCK ACTUATOR - REPLACE |  | K7549 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 7.1 | 7.1 | 7.1 | 7.1 | 7.1 | 7.1
ENGINE CODE 4 | R |  | -- | -- | -- | 5.0 | 5.0 | 5.0
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CARRIER ASSEMBLY, REACTION - REPLACE |  | K7565 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.2 | 9.2 | 9.2 | 9.2 | 9.2 | 9.2
ENGINE CODE 4 | R |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CLUTCH ASSEMBLY, REVERSE INPUT - R&R OR REPLACE |  | K7571 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.4 | 9.4 | 9.4 | 9.4 | 9.4 | 9.4
ENGINE CODE 4 | R |  | -- | -- | -- | 8.5 | 8.5 | 8.5
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

BAND, INTERMEDIATE/4TH - REPLACE |  | K7573 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.0 | 9.0 | 9.0 | 9.0 | 9.0 | 9.0
ENGINE CODE 4 |  |  | -- | -- | -- | 8.1 | 8.1 | 8.1
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

SUPPORT, FORWARD CLUTCH - REPLACE |  | K7577 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 |  |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CLUTCH ASSEMBLY, DIRECT AND COAST - R&R OR REPLACE |  | K7581 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.8 | 9.8 | 9.8 | 9.8 | 9.8 | 9.8
ENGINE CODE 4 |  |  | -- | -- | -- | 8.9 | 8.9 | 8.9
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

HOUSING, DIRECT & COAST CLUTCH & INPUT SHAFT - REPLACE |  | K7582 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.8 | 9.8 | 9.8 | 9.8 | 9.8 | 9.8
ENGINE CODE 4 |  |  | -- | -- | -- | 8.9 | 8.9 | 8.9
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

GEAR, INPUT INTERNAL AND FORWARD CLUTCH HUB - REPLACE |  | K7583 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.2 | 9.2 | 9.2 | 9.2 | 9.2 | 9.2
ENGINE CODE 4 |  |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CLUTCH, LO ROLLER - REPLACE |  | K7584 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.4 | 9.4 | 9.4 | 9.4 | 9.4 | 9.4
ENGINE CODE 4 |  |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CARRIER, INPUT - REPLACE |  | K7590 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.1 | 9.1 | 9.1 | 9.1 | 9.1 | 9.1
ENGINE CODE 4 |  |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

GEAR, REACTION INTERNAL - REPLACE |  | K7594 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.1 | 9.1 | 9.1 | 9.1 | 9.1 | 9.1
ENGINE CODE 4 |  |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

BAND, LO/REVERSE - REPLACE |  | K7596 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.2 | 9.2 | 9.2 | 9.2 | 9.2 | 9.2
ENGINE CODE 4 |  |  | -- | -- | -- | 8.3 | 8.3 | 8.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

DIFFERENTIAL AND FINAL DRIVE ASSEMBLY, TRANSAXLE - REPLACE |  | K7620 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 |  |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

DIFFERENTIAL AND FINAL DRIVE ASSEMBLY, TRANSMISSION - R&R |  | K7629 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 |  |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

DIFFERENTIAL AND FINAL DRIVE ASSEMBLY, TRANSMISSION - R&R |  | K7629 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 |  |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

GEAR, FINAL DRIVE INTERNAL - R&R OR REPLACE |  | K7750 |  |  |  |  |  |

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 9.5 | 9.5 | 9.5 | 9.5 | 9.5 | 9.5
ENGINE CODE 4 |  |  | -- | -- | -- | 8.6 | 8.6 | 8.6
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

CASE, TRANSAXLE - REPLACE

- PART GP: 4.103

K7800

- ATTENTION: The following "NOTE" has been deleted from this labor operation.

- "NOTE" For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

ENGINE CODES D & T |  |  | 10.1 | 10.1 | 10.1 | 10.1 | 10.1 | 10.1
ENGINE CODE 4 | R |  | -- | -- | -- | 9.3 | 9.3 | 9.3
ADD: |  |  |  |  |  |  |  |

- A- With A/C (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- NOTE: No Change to Remaining "ADD" Conditions.

*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.2

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

COMPRESSOR ASSEMBLY - REPLACE

- PART GP: 9.170

D4440

1.2

1.2

1.2

1.2

1.2

1.2

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

0.5

0.5

0.5

0.5

0.5

- B- To Install Liquid Line Filter (THIS "ADD" CONDITION HAS BEEN DELETED).

R

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.2

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

BEARING AND HUB ASSEMBLY, FRONT WHEEL - REPLACE

- PART GP: 6.307

- INC: R&R Caliper with Bracket, Rotor and Dust Shield

R

E2320

RIGHT |  |  | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
LEFT |  | E2321 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
BOTH |  | E2327 | 1.5 | 1.5 | 1.7 | 1.7 | 1.7 | 1.7
SENSOR, CRANKSHAFT POSITION - REPLACE

- No Change to "ADD" Condition

R

J4355

0.4

0.4

0.3

0.3

0.9

0.9

SWITCH, EVAPORATIVE EMISSION CANISTER PURGE THERMAL VACUUM - REPLACE |  | J6335 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
VALVE, EVAPORATIVE EMISSION CANISTER PURGE VACUUM - REPLACE |  | J6441 | -- | -- | 0.2 | 0.2 | 0.2 | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - M Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
VALVE, EVAPORATOR EMISSION CANISTER CONTROL - REPLACE |  | J6324 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE | R | J6441 | -- | -- | 1.6 | 1.6 | 1.6 | 1.6
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System Without C69, Rear Auxiliary A/C

0.5

- B- Recover/Recharge A/C System With C69, Rear Auxiliary A/C

0.7

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

Without C69, Rear Auxiliary A/C | -- | -- | -- | -- | -- | 0.5
With C69, Rear Auxiliary A/C | -- | -- | -- | -- | -- | 0.6
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System Without C69, Rear Auxiliary A/C

0.5

- B- Recover/Recharge A/C System With C69, Rear Auxiliary A/C

0.7

TOE, FRONT - ADJUST

- NOTE: No Change to existing "NOTES"

R

E2000

M-VAN |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
L-VAN |  |  | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
ROD, STEERING RELAY - REPLACE

- PART GP: 6.870

E7980

0.5

0.5

0.5

0.5

0.5

0.5

- NOTE: For check and adjust toe-in, refer to operation E2000 and add the applicable time to the regular hours column.

N

ADD: | R |  |  |  |  |  |  |

- A- To Adjust Toe-In

- (THIS "ADD" CONDITION HAS BEEN DELETED)

TIE ROD, INNER - REPLACE

- PART GP: 6.230

- NOTE: For check and adjust toe-in, refer to operation E2000 and add the applicable time to the regular hours column.

N

RIGHT |  | E8040 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
LEFT |  | E8041 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
BOTH |  | E8047 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
ADD: | R |  |  |  |  |  |  |

- A- To Adjust Toe-In

- (THIS "ADD" CONDITION HAS BEEN DELETED)

TIE ROD END AND/OR ADJUSTER SLEEVE - REPLACE

- PART GP: 6.233

- NOTE: For check and adjust toe-in, refer to operation E2000 and add the applicable time to the regular hours column.

N

RIGHT |  | E8060 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
LEFT |  | E8061 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
BOTH |  | E8067 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
ADD: | R |  |  |  |  |  |  |

- A- To Adjust Toe-In

- (THIS "ADD" CONDITION HAS BEEN DELETED)

PLUG, TRANSFER CASE DRAIN - REPLACE | R | K4290 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
PLUG, TRANSFER CASE FILL - REPLACE | N | K4291 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
LOCK, COMPARTMENT (INSTRUMENT PANEL) - REPLACE

- PART GP: 10.266

C2100

MALIBU & CUTLASS |  |  | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
GRAND AM & ALERO | R |  | 0.2 | 0.2 | 0.2 | 0.6 | 0.6 | 0.6
ACHIEVA & SKYLARK |  |  | 0.2 | 0.2 | 0.2 |  |  |

- No Change to "ADD" Condition

FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.5
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.5

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

CORE, EVAPORATOR - REPLACE |  | D3320 |  |  |  |  |  |
MALIBU & CUTLASS | R |  | -- | 4.9 | 4.9 | 4.9 | 4.9 | 4.9
GRAND AM & ALERO |  |  | 2.1 | 2.1 | 2.1 | 1.3 | 1.3 | 1.3
ACHIEVA - 4 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
ACHIEVA - 6 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
SKYLARK - 4 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
SKYLARK - 6 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

R

0.5

0.5

0.5

0.5

0.5

0.5

INSULATOR AND/OR SUPPORT, REAR STABILIZER SHAFT - REPLACE

- PART GP: 7.243

- NOTE: No Change to Labor Operations E4180 or E4181

BOTH |  | E4187 |  |  |  |  |  |
MALIBU & CUTLASS | R |  | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
GRAND AM & ALERO |  |  | -- | -- | -- | 0.3 | 0.3 | 0.3
GEAR ASSEMBLY, POWER STEERING - R&R |  | E9720 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
GEAR ASSEMBLY, POWER STEERING - REPLACE

- PART GP: 6.508

- INC: Transfer outer tie rods.

- NOTE: For check and adjust toe-in, refer to Operation E2000 and add the applicable times to the regular hours column.

N

E9740

ACHIEVA & SKYLARK |  |  | 1.2 | 1.2 | 1.2 | 1.2 |  |
GRAND AM & ALERO |  |  | 1.2 | 1.2 | 1.2 | 1.7 | 1.7 | .17
MALIBU & CUTLASS |  |  | -- | 1.7 | 1.7 | 1.7 | 1.7 | 1.7
CYLINDER, BRAKE MASTER - REPLACE

- PART GP: 4.650

H0640

MALIBU & CUTLASS |  |  | -- | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
ACHIEVA & SKYLARK |  |  | 1.2 | 1.2 | 1.2 |  |  |
GRAND AM & ALERO | R |  | 1.2 | 1.2 | 1.2 | 1.0 | 1.0 | 1.0
MOTOR PACK (ABS) - REPLACE | R | H2506 | 0.6 | 2.0 | 2.0 | 2.0 | 2.0 | 2.0

- No Change to "ADD" Condition

BOOT, PARKING BRAKE HANDLE - REPLACE | N | H2815 | -- | -- | -- | 0.8 | 0.8 | 0.8
WIRES, SPARK PLUG - REPLACE

- No Change to "PART GP", or "POLICY"

ONE |  | J4206 |  |  |  |  |  |
EXC ENGINE CODE M, E and J |  |  | 0.2 | 0.2 | 0.2 |  |  |
ENGINE CODE M, E and J |  |  | 0.2 | 0.2 | 0.2 | 0.3 | 0.3 | 0.3

- No Change to "ADD" Conditions

SENSOR, CAMSHAFT POSITION - REPLACE

- POLICY: E

J4350

4 CYL |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
6 CYL | R |  | 0.8 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE | R | J6441 | 0.2 | 0.2 | 0.2 | 0.3 | 0.3 | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised |  |  |  |  |  |  |

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ARM, STEERING IDLER - REPLACE

- PART GP: 6.895

- NOTE: For alignment times refer to operation E2000 and add applicable times to the regular hours column.

R

E7960

S TRUCK |  |  | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
T TRUCK |  |  | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
ADD: | R |  |  |  |  |  |  |

- A- W/Skid Plate

--

--

0.2

0.2

0.2

0.2

- B- To Adjust Toe-In

- (THIS "ADD" CONDITION HAS BEEN DELETED).

ROD, STEERING RELAY - REPLACE

- PART GP: 6.870

- NOTE: For alignment times refer to operation E2000 and add applicable times to the regular hours column.

R

E7980

0.6

0.6

0.6

0.6

0.6

0.6

ADD: | R |  |  |  |  |  |  |

- A- To Adjust Toe-In

- (THIS "ADD" CONDITION HAS BEEN DELETED).

TIE ROD END AND/OR ADJUSTER SLEEVE - REPLACE

- PART GP: 6.230

- NOTE: For alignment times refer to operation E2000 and add applicable times to the regular hours column.

R

RIGHT |  | E8040 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
LEFT |  | E8041 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
BOTH |  | E8047 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
TIE ROD END AND/OR ADJUSTER SLEEVE - REPLACE

- PART GP: 6.233

- NOTE: For alignment times refer to operation E2000 and add applicable times to the regular hours column.

R

RIGHT |  | E8060 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
LEFT |  | E8061 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
BOTH |  | E8067 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
*IND: N - New/R - Revised |  |  |  |  |  |  |

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System Without C69, Rear Auxiliary A/C

0.5

- B- Recover/Recharge A/C System With C69, Rear Auxiliary A/C

0.7

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

0.4

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System Without C69, Rear Auxiliary A/C

0.5

- B- Recover/Recharge A/C System With C69, Rear Auxiliary A/C

0.7

SUPPORT AND SEALS, DRIVE SPROCKET - REPLACE

- NOTE: Applies to Auto Trans 4T65E

N

K7522

--

--

--

9.8

9.8

9.8

ADD: |  |  |  |  |  |  |  |

- A- To Recondition 3-4 Accumulator

--

--

--

0.2

0.2

0.2

- B- To Clean and Recondition Valve Body

--

--

--

1.0

1.0

1.0

- C- To Recondition Oil Pump

--

--

--

0.4

0.4

0.4

- D- To Recondition Trans Completely (Exc Carrier/Diff Final Drive)

--

--

--

4.2

4.2

4.2

- E- To Recondition Carrier/Differential Final Drive Assembly

--

--

--

0.8

0.8

0.8

- F- To Clean Parts On Vehicle Over 30,000 Miles/48,000 Kilometers If Nec

--

--

--

0.5

0.5

0.5

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MODULE, BLOWER MOTOR CONTROL - REPLACE | R | D0890 | -- | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.5
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

CHEVROLET, PONTIAC, BUICK |  |  |  |  |  |  |  | 0.8
OLDSMOBILE |  |  |  |  |  |  |  | 2.2
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

COMPRESSOR ASSEMBLY - REPLACE

- PART GP: 9.170

D4440

ENGINE CODE H |  |  | -- | -- | -- | 2.1 | 2.1 | 2.1
ENGINE CODE K AND 1 |  |  | 0.8 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
ENGINE CODE X |  |  | 1.1 | 1.1 |  |  |  |
ENGINE CODE M, T, J AND E |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

0.5

0.5

0.5

0.5

0.5

- B- To Install Liquid Line Filter (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- C- To Install Liquid Line With Filter (THIS "ADD" CONDITION HAS BEEN DELETED).

R

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

GEAR ASSEMBLY, POWER STEERING - REPLACE

- PART GP: 6.508

- NOTE: For check and adjust toe-in, refer to Operation E2000 and add the applicable times to the regular hours column.

N

E9740

ENGINE CODE M, T, J, E, K, 1, H |  |  | 2.0 | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
ENGINE CODE X |  |  | 2.6 | 2.6 |  |  |  |
SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BBEN DELETED FROM ALL APPLICABLE YEARS
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE |  | J6441 | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FILTER, IN-LINE A/C - REPLACE | N | D3255 |  |  |  |  |  | 0.4
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

FILTER, IN-LINE A/C - INSTALL

- NOTE: This Labor Operation can only be used with a Compressor Replacement D4440.

N

D3258

2.1

ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

PULLEY, CRANKSHAFT BALANCER - REPLACE

- NOTE: Applies to V8 Engine, Codes G, P and 5

- No Change to "NOTE" or "ADD" Condition

R

J0710

1.3

2.1

2.1

2.3

2.3

2.3

SOLENOID, EVAPORATIVE EMISSION CANISTER VENT CONTROL - REPLACE |  | J6391 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE | N | J6441 | 0.4 |  |  |  |  |
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

0-0.3

*IND: N - New/R - Revised