For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the cap from the wiper motor (1) spindle.
3. Remove the nut from the wiper motor (1) spindle.
4. Remove the wiper arm.
5. Remove the nut from the wiper motor (1) spindle.
6. Remove the following components from the wiper motor (1) spindle:

• | The grommet

• | The washer

7. Open the liftgate (3).
8. Remove the trim panel. Refer to Liftgate Finish Trim Panel.
9. Remove the wiper motor (1) to liftgate bolts/screws (2).
10. Remove the wiper motor (1).

### Installation Procedure

1. Install the wiper motor (1) to the liftgate (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the wiper motor (1) to liftgate bolts/screws (2).

Tighten
Tighten the bolts/screws to 5.5 N·m (49 lb in).

3. Install the trim panel. Refer to Liftgate Trim Finish Panel.
4. Close the liftgate (3).
5. Install the following components to the wiper motor (1) spindle:

• | The grommet

• | The washer

6. Install the nut to the wiper motor (1) spindle.

Tighten
Tighten the nut to 25 N·m (18 lb in).

7. Install the cap to the wiper motor (1) spindle.
8. Connect the negative battery cable.