For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
2. Carefully peel the water deflector from the door.

### Installation Procedure

Important: A proper adhesive bond between the sliding door deflector and the inner panel will prevent water leaks.

1. Install the water deflector to the door. Use a roller in order to properly set the adhesive to the door panel.
2. Install the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .