For 1990-2009 cars

### Removal Procedure

1. Remove the right rear quarter lower trim panel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.
2. Pull the alarm (4) from power sliding door actuator motor, separating the hook and loop retainer.
3. Remove the alarm electrical connector.

### Installation Procedure

1. Connect the alarm electrical connector.
2. Push the alarm (4) onto the power sliding door actuator motor, securing the hook and loop retainer.
3. Install the right rear quarter lower trim panel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.