For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster panel. Refer toKnee Bolster Replacement in Instrument Panel, Gages and Console.
2. Remove the EBCM/EBTCM electrical connectors (4).
3. Use pressure tabs in order to release the EBCM/EBTCM (1) from the EBCM/EBTCM bracket (2).

### Installation Procedure

1. Slide the EBCM/EBTCM (1) into the EBCM/EBTCM bracket (2) until pressure tabs secure the EBCM/EBTCM.
2. Install the EBCM/EBTCM electrical connectors (4).
3. Install the knee bolster panel. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.