For 1990-2009 cars

### Removal Procedure

1. Open and suitably support the hood.
2. Disconnect the hood release cable. Refer to Hood Primary Latch Release Cable Replacement .
3. Remove the bolts/screws from the primary hood latch at the latch support bracket.
4. Remove the primary hood latch from the support bracket.

### Installation Procedure

1. Install the primary hood latch support bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts/screws to the primary hood latch at the latch support bracket.

Tighten
Tighten the bolts/screws to 25 N·m (18 lb ft).

3. Connect the hood release cable. Refer to Hood Primary Latch Release Cable Replacement .
4. Adjust the hood. Refer to Hood Adjustment .