For 1990-2009 cars

### Automatic Door Lock Operation Modes

• | Shift out of PARK lock enabled (modes 2, 3 and 4): Locks all doors when shifting the transaxle out of PARK with the driver's door closed.

• | Ignition OFF unlock enabled (mode 3): Unlocks all doors when turning the ignition switch from the RUN to the UNLOCK position.

• | Shift into PARK unlock enabled (mode 4): Unlocks all doors when shifting the transaxle into PARK.

### Changing the Automatic Door Lock Operation Mode

Perform the following procedure to change the automatic door lock operation mode:

1. Turn off the IP dimmer switch.
2. Turn the ignition switch to the LOCK position.
3. Remove the BCM PRGRM fuse.
4. Turn the ignition switch to the ACC position.

• | The BCM sounds the chime a number of times equivalent to the BCM type installed on the vehicle (1, 2, 3, or 4 chimes).

• | Now the BCM has entered the feature customization mode.

5. To change the automatic door lock operation mode, press and release the LOCK on either door lock switch.

• | The BCM sounds the chime a number of times equivalent to the automatic door lock operation mode.

• | A transition past mode 4 repeats the sequence starting with mode 1.

The automatic door lock operation modes are as follows:

MODE | Shift Out Of Park Lock | Ignition Off Unlock | Shift Into Park Unlock
--- | --- | --- | ---
1 | Disabled | Disabled | Disabled
2 | Enabled | Disabled | Disabled
3 | Enabled | Enabled | Disabled
4 | Enabled | Disabled | Enabled

To exit and save the current customization mode:

1. Turn the ignition switch to the lock position.
2. Reinstall the BCM PRGRM fuse.

If unable to change lock modes, refer to Feature Customization Mode Inoperative for diagnosis and repair.

### Locking Control Modes

• | Last door closed locking enabled (modes 3 and 4): When pressing LOCK on either door lock switch with the ignition switch in the LOCK position, this mode locks all doors five seconds after closing all vehicle doors.

• | Lockout prevention enabled (modes 2 and 4): When pressing LOCK on either door lock switch with the key in the ignition cylinder and the driver's door is open, the BCM does not lock the doors.

### Changing the Locking Control Mode

Perform the following procedure to change the locking control mode:

1. Turn off the IP dimmer switch.
2. Turn the ignition switch to the LOCK position.
3. Remove the BCM PRGRM fuse.
4. Turn the ignition switch to the ACC position.

• | The BCM sounds the chime a number of times equivalent to the BCM type installed on the vehicle (1, 2, 3, or 4 chimes).

• | Now the BCM has entered the feature customization mode.

5. To change the locking control mode; press and release the UNLOCK on either door lock switch.

• | The BCM sounds the chime a number of times equivalent to the locking control mode.

• | A transition past mode 4 repeats the sequence starting with mode 1.

The locking control modes are as follows:

Mode | Last Door Closed Locking | Lockout Prevention
--- | --- | ---
1 | Disabled | Disabled
2 | Disabled | Enabled
3 | Enabled | Disabled
4 | Enabled | Enabled

To exit and save the current customization mode:

1. Turn the ignition switch to the LOCK position.
2. Reinstall the BCM PRGRM fuse.

If unable to change locking modes, refer to Feature Customization Mode Inoperative for diagnosis and repair.