For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
CD Player | Center of the IP floor console | -- | Entertainment Connector End Views in Entertainment Systems
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Driver Information Display | In the roof console | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Electronic Brake Control Module/Electronic Brake Traction Control Module (EBCM/EBTCM) | Left side of the IP, above the parking cable bracket | Antilock Brake System Component Views in Antilock Brakes Systems | Antilock Brake System Connector End Views in Antilock Brakes Systems
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | --
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Below the right front seat | SIR Component Views in SIR | SIR Connector End Views in SIR
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Cotnrols
Radio | Center of the IP console | Entertainment Component Views in Entertainment Systems | Entertainment Connector End Views in Entertainment Systems
C101 (10 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C103 and C181 | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C308 (23 cavities) | Body wiring harness to the dome lamp wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views | Inline Harness Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
S211 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and the rear widow wiper/washer multifunction switch breakout | -- | --
S237 | IP harness, right side of the IP approximately 4 cm (2 in) from the C203 breakout | -- | --
S312 | Body harness, front of the right B-pillar approximately 31 cm (12 in) front of the inflatable restraint sensing and diagnostic module breakout | -- | --
S328 | Body harness, between the left D-pillar and the wheel well approximately 32 cm (13 in) forward of the G401 breakout | -- | --