For 1990-2009 cars

### Removal Procedure

For proper routing and replacement of canister hoses, refer to Emission Hose Routing Diagram. When replacing hoses, use 6148M or equivalent.

1. Disconnect the EVAP lines.

Be sure to mark the EVAP lines for correct installation.

2. Remove the EVAP Canister retainer Bolt.
3. Remove the EVAP Canister.

### Installation Procedure

1. Install the EVAP Canister
2. Install the EVAP Canister retainer bolt.
3. Install the lines to the EVAP canister.

Be sure to Install the lines to the correctly