For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Power Windows System Check performed? | -- | Go to Step 2 | Go to Power Windows System Check
2 |

1. Turn the ignition switch to the RUN position.
2. Using a test lamp, backprobe the left front window switch connector from terminal H to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Using a test lamp, backprobe the left front window switch connector between terminal H and terminal G. Does the test lamp light? | -- | Go to Step 5 | Go to Step 6
4 |

1. Test for a poor connection at C200 terminal A8.
2. If OK, repair the open in CKT 141, between PWR WDO circuit breaker and S307.

Is the repair complete?

--

Go to Step 7

--

5 | Replace the left front window switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 7 | --
6 | Repair the open in CKT 750, between left front window switch assembly connector terminal G and S504. Is the repair complete? | -- | Go to Step 7 | --
7 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Power Windows System Check

--