For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check the vehicle for Diagnostic Trouble Codes (DTC). Are there any DTC codes? | -- | Go to Diagnostic Trouble Code (DTC) List in Antilock Brake System | Go to Step 2
2 |

1. Disconnect the Electronic Brake Traction Control Module (EBTCM) connector C1.
2. Turn the ignition switch to the RUN position.

Is the LOW TRACTION indicator on?

--

Go to Step 3

Go to Step 4

3 |

1. Using a J 39200 digital multimeter (DMM), check for a short to ground in CKT 832.
2. If OK, replace the instrument cluster. Refer to Instrument Cluster Replacement .

Has the repair been made and the system rechecked?

--

System OK

--

4 |

1. Turn the ignition switch to the RUN position.
2. Connect a fused (3-amp) jumper between the EBTCM harness connector C1 terminal A6 and ground.

Is the LOW TRACTION indicator on?

--

Go to Step 5

Go to Step 6

5 | A fault exists in the EBTCM or the ABS. Refer to Diagnostic System Check in Antilock Brake System for diagnosis. as the repair been made and the system rechecked? | -- | System OK | --
6 |

1. Check for a poor connection or an open in CKT 832 between the instrument cluster connector C1 terminal F and the EBTCM harness connector C1 terminal A6.
2. If OK, replace the instrument cluster. Refer to Instrument Cluster Replacement .

Has the repair been made and the system rechecked?

--

System OK

--