For 1990-2009 cars

Table 1: | Ambient Air Temperature Sensor
Table 2: | Brake Fluid Level Indicator Sensor
Table 3: | Driver Information Display
Table 4: | Engine Coolant Level Indicator Module
Table 5: | Engine Oil Level Indicator Switch
Table 6: | Instrument Cluster C1
Table 7: | Instrument Cluster C2
Table 8: | Traction Control Module Malfunction Indicator Lamp

#### Ambient Air Temperature Sensor

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRN/BLK | 735 | Ambient air temperature sensor signal
B | BLK | 1550 | Ground

#### Brake Fluid Level Indicator Sensor

Connector Part Information |

• | 12162194

• | 2-Way F Metri-Pack 150.2 Series Sealed, P2S (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1450 | Ground
B | TAN/WHT | 33 | Brake warning indicator lamp output

#### Driver Information Display

Connector Part Information |

• | 12064980

• | 9-Way Female MIC/P 100 (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | YEL | 43 | Fused accessory feed
8 | BLK | 1550 | Ground
9 | DK GRN | 389 | Vehicle speed signal
10 | LT GRN/BLK | 735 | Ambient air temperature sensor signal
11 | GRY | 8 | Interior lamp dim signal
12 | GRY/BLK | 308 | Parklamp switch output - parklamps ON
13 | YEL | 136 | Fuel level input
14 | ORN | 640 | Fused battery feed
15 | TAN | 800 | UART serial data communication

#### Engine Coolant Level Indicator Module

Connector Part Information |

• | 12162185

• | 3-Way F Metri-Pack 150.2 Series Sealed, Pull to Seat (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | YEL/BLK | 68 | Low coolant indicator lamp output
C | BLK/WHT | 451 | PCM ground

#### Engine Oil Level Indicator Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1174 | Engine oil level indicator input
B | BLK/WHT | 451 | Ground

#### Instrument Cluster C1

Connector Part Information |

• | 12129406

• | 18-Wedge P/C BOW Pull to Seat (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 31 | Oil pressure indicator lamp output
B | TAN/WHT | 33 | Brake warning indicator lamp output
C | YEL | 772 | Transaxle range switch input B
D | WHT | 776 | Transaxle range switch parity input
E | DK GRN | 35 | Coolant temperature indicator lamp output
F | LT BLU | 832 | Low traction indicator output
G | YEL | 804 | Door ajar indicator lamp output
H | BRN/WHT | 1173 | Low oil level indicator lamp output
I | PNK | 39 | Fused ignition 1 feed
J | BLK/WHT | 771 | Transaxle range switch input A
K | PNK | 1020 | Fused ignition 0 feed
L | GRY/BLK | 308 | Parklamp switch output - parklamps ON
M | PNK | 39 | Fused ignition 1 feed
N | LT GRN | 867 | Antilock warning indicator lamp output
O | DK GRN | 135 | Engine coolant temperature output
P | ORN | 55 | Fuel level input
Q | -- | -- | Not Used
R | BRN/WHT | 419 | Check engine indicator lamp output

#### Instrument Cluster C2

Connector Part Information |

• | 12129405

• | 18-Wedge P/C BOW Pull to Seat (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 1808 | TCS indicator signal - warning
B | -- | -- | Not Used
C | YEL/BLK | 68 | Low coolant indicator lamp output
D | BLK | 1550 | Ground
E | -- | -- | Not Used
F | BRN | 358 | SIR indicator control
G | -- | -- | Not Used
H | WHT | 121 | Tachometer signal
I | GRY | 8 | Interior lamp dim signal
J | -- | -- | Not Used
K | BRN | 25 | Charge indicator lamp
L | DK GRN/WHT | 529 | Seat belt indicator lamp feed
M | GRY | 773 | Transaxle range switch input C
N | DK GRN | 389 | Vehicle speed signal
O | BLK | 1450 | Ground
P | YEL | 18 | Tail/turn/stoplamp feed - left rear
Q | LT GRN | 11 | High beam headlamp feed
R | DK GRN | 19 | Tail/stop/stoplamp feed - right rear

#### Traction Control Module Malfunction Indicator Lamp

Connector Part Information |

• | 12015410

• | Printed Circuit Connector Edgeboard Series Standard (Green)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | PNK | 39 | Fused ignition 1 feed
C | PPL/WHT | 1572 | TCS warning indicator lamp
D | BLK | 1550 | Ground
E | WHT | 1808 | TCS indicator signal - warning
F | -- | -- | Not Used