For 1990-2009 cars

# SLIDING SIDE DOOR RATTLES (INSTALL BRACKETS)

#### SUBJECT: SLIDING SIDE DOOR RATTLES (INSTALL NEW BRACKETS)

#### MODELS: 1990-94 CHEVROLET LUMINA 1990-94 OLDSMOBILE SILHOUETTE 1990-94 PONTIAC TRANS SPORT

#### CONDITION:

SOME CUSTOMERS MAY COMMENT THE SLIDING SIDE DOOR RATTLES OVER ROUGH ROADS.

#### CAUSE:

UPPER AND LOWER ROLLER BRACKETS HAVE STEEL ROLLERS WHICH RATTLE IN THE TRACKS.

#### CORRECTION:

INSTALL NEW UPPER AND LOWER ROLLER BRACKETS WHICH HAVE HYTREL ROLLERS.

#### IMPORTANT: THE UPPER AND LOWER ROLLER BRACKET ASSEMBLIES SHOULD BE CHANGED AFTER YOU HAVE CONFIRMED THAT THE DOOR ALIGNMENT, STRIKER AND THE FRONT GUIDE PINS TO POCKETS ARE IN ALIGNMENT AND NOT BINDING.

LOWER ROLLER BRACKET EXCEPT ELECTRIC SLIDING DOOR - P/N 10262759 LOWER ROLLER BRACKET ELECTRIC SLIDING DOOR - P/N 10264978 UPPER ROLLER BRACKET MANUAL OR POWER - P/N 10262752

#### PART AVAILABILITY:

PARTS ARE EXPECTED TO BE AVAILABLE ON 11/21/94 AT GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: B5020 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.