For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat. Refer to Rear Seat Replacement .
2. Unhook the J retainer on the bottom edge of the seat back cover.
3. Reach underneath the seat back cover.
4. Release the C-clip from the armrest pivot shaft while pushing in on the armrest.
5. Remove the armrest from the seat.

### Installation Procedure

1. Install the armrest to the seat.

Important: During the removal of the armrest, ensure that you reset the C-clip (open end facing down) into the slotted shaft if the armrest C-clip disengages from the slotted shaft.

2. Press firmly inward on the armrest in order to seat the C-clip onto the armrest pivot shaft.
3. Hook the J retainer at the bottom edge of the seat back cover.
4. Install the rear seat. Refer to Rear Seat Replacement .
5. Reposition the seat back to the original position.