For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left front tire and wheel. Refer to Wheel Removal in Tires and Wheels.
3. Remove the left and right stabilizer shaft insulators and brackets . Refer to Stabilizer Shaft Insulator Replacement
4. Remove the left and right stabilizer shaft links. Refer to Stabilizer Shaft Link Replacement
5. Remove the stabilizer shaft from the left side of the vehicle.

### Installation Procedure

1. Install the stabilizer shaft from the left side of the vehicle.
2. Install the left and right stabilizer shaft links. Refer to Stabilizer Shaft Link Replacement
3. Install the left and right stabilizer shaft insulators and brackets. Refer to Stabilizer Shaft Insulator Replacement
4. Install the left front tire and wheel. Refer to Wheel Installation in Tires and Wheels.
5. Lower the vehicle.