For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Shift the transaxle into the PARK position.
2. Turn the ignition switch to the RUN position.
3. Disconnect the transaxle range switch connector C1.

Did the backup lamps light?

--

Go to Step 3

Go to Step 2

2 |

1. Adjust or replace the transaxle range switch. Refer to Park/Neutral Position Switch Replacement
2. Inspect the system.

Is the repair complete?

--

System OK

--

3 |

1. Repair a short to B+ on CKT 24.
2. Inspect the system.

Is the repair complete?

--

System OK

--