For 1990-2009 cars

### Removal Procedure

Important: The solid-type head restraint is the only head restraint with a serviceable trim cover.

1. Pull the head restraint to the full up position.
2. Disconnect the J and arrow retainers at the bottom of the cover.
3. Remove the head restraint cover.

### Installation Procedure

1. Install the head restraint cover.
2. Connect the J and arrow retainers at the bottom of the cover.
3. Return the head restraint to its original position.