For 1990-2009 cars

### Removal Procedure

1. Remove the left side rear quarter trim pannel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.
2. Remove the blower motor electrical connector (2).
3. Lift the tabs on the blower motor. Turn the blower motor counterclockwise.
4. Remove the blower motor.

### Installation Procedure

1. Install the blower motor.
2. Turn the blower motor clockwise until the tabs lock into position.
3. Connect the electrical connector (2) to the blower motor.
4. Install the left side rear quarter trim pannel. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.