For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body air inlet duct. Refer to Air Cleaner Element Replacement in Engine Controls-3.4L.
2. Remove the automatic transaxle range selector cable from the automatic transaxle range selector lever.
3. Remove the automatic transaxle range selector cable from the automatic transaxle range selector cable bracket.
4. Remove the steering column opening filler.
5. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.
6. Remove the automatic transaxle range selector cable from the column control lever.
7. Remove the automatic transaxle range selector cable from the steering column bracket.
8. Remove the automatic transaxle range selector cable through the hole in the cowl.

### Installation Procedure

1. Properly route the automatic transaxle range selector cable through the engine compartment.
2. Properly route the automatic transaxle range selector cable through the cowl.
3. Install the automatic transaxle range selector cable to the steering column bracket.
4. Install the automatic transaxle range selector cable to the column control lever.
5. Install the steering column opening filler.
6. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.
7. Install the automatic transaxle range selector cable to the automatic transaxle range selector cable bracket.
8. Install the automatic transaxle range selector cable to the automatic transaxle range selector lever.
9. Adjust the automatic transaxle range selector cable if necessary. Refer to Automatic Transmission Range Selector Cable Adjustment .
10. Install the throttle body air inlet duct. Refer to Air Cleaner Element Replacement in Engine Controls-3.4L.