For 1990-2009 cars

### Removal Procedure

1. Open the sliding door.
2. Remove the bolt/screw from the fuel filler interlock bracket.
3. Slide the fuel filler interlock bracket toward the front of the vehicle.
4. Remove the fuel filler interlock from the body.
5. Disconnect the fuel filler interlock cable from the fuel filler interlock bracket.

### Installation Procedure

1. Connect the fuel filler interlock cable to the fuel filler interlock bracket.
2. Insert the fuel filler interlock into the proper hole in the body.
3. Slide the fuel filler interlock bracket toward the rear of the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the bolt/screw to the fuel filler interlock bracket.

Tighten
Tighten the bolt/screw to 25 N·m (18 lb ft).

5. Close the sliding door.