For 1990-2009 cars

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Remove both sides of the rear quarter trim. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.
3. Disconnect the electrical connectors.
4. Remove the retainers from the body.
5. Remove the harness from the body.

### Installation Procedure

1. Route the harness into the body.
2. Install the retainers to the body.
3. Connect the electrical connectors.
4. Install both sides of the rear quarter trim. Refer to Rear Quarter Lower Trim Panel Replacement in Interior Trim.
5. Install the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.