For 1990-2009 cars

# REVISED:SECTION 8E - TOOL REVISION

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTION 8E - TOOL REVISION FOR WINDSHIELD WIPER ARM REMOVAL

#### MODELS: 1990-95 CHEVROLET LUMINA APV 1990-95 OLDSMOBILE SILHOUETTE 1990-95 PONTIAC TRANSPORT

THIS BULLETIN CONTAINS REVISIONS TO SECTION 8E.

SECTION 8E-8 "WIPER ARM REPLACEMENT" PROCEDURE SHOULD READ "REMOVE WIPER ARM ASSEMBLY FROM DRIVE SHAFT USING PULLER J-22888-20A, WITH (-50) LEGS AND (-90) TIP, SEE ATTACHED ILLUSTRATION.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.