For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 3C STEERING KNUCKLE NUT FASTENING

#### Subject: SERVICE MANUAL UPDATE - SECTION 3C - STEERING KNUCKLE NUT FASTENING TORQUE Models Affected: 1992-93 TRANS SPORT MODELS

This bulletin serves to cancel and supersede the steering knuckle nut (305) torque specifications presently published in Section 3C of the 1992-93 Trans Sport Service Manuals.

The correct steering knuckle nut (305) fastening torque for 1992-93 vehicles is 76 N.m (56 lb.ft.) (Figure 1).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.