For 1990-2009 cars

# REMOTE MIRROR CONTROL KNOB LOOSE MANUAL/ELECT INST CLIPS

#### SUBJECT: REMOTE MIRROR CONTROL KNOB LOOSE - MANUAL/ELECTRIC (INSTALL RETAINING CLIPS)

#### MODELS AFFECTED: 1990-92 TRANS SPORT MODELS

#### CONDITION:

---------- Some owners of 1990-92 Trans Sport models may experience a condition where the control knob for the outside rear view mirror is loose in the door upper trim garnish molding. This condition may occur on the left and/or right side.

#### CORRECTION:

----------- Install (4) four retaining clips, P/N 10215107, using the following procedure:

1. Remove door trim and upper garnish molding.

2. Remove outside mirror control from the garnish molding by loosening the set screw.

3. Install the first clip (P/N 10215107) as close to set screw location as possible. (See Illustration). The remaining (3) three clips are to be positioned at 90 degrees from each other around the opening.

4. Reinstall mirror control to the garnish molding, tighten set screw, and replace lower trim panel.

#### PART AVAILABILITY:

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operations: Right - C-3210, Left - C-3211 Use Applicable Labor Times.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.