For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Has the Park Brake System Check been performed? | -- | Go to Step 2 | Go to Park Brake System Check
2 | Inspect the park brake cables for binding. Replace as necessary. Has the inspection/repair been completed? | -- | Go to Step 5 | --
3 | Ensure that the park brake cable is adjusted properly. Adjust the park brake cable as needed. Refer to Park Brake Cable Service/Adjustment . Has the inspection/repair been completed? | -- | Go to Step 5 | --
4 |

1. Inspect the rear brake shoe lining/park brake lining for excessive wear. Replace as necessary.
2. Ensure that the park brake actuator does not bind and operates freely. Repair or replace as necessary.
3. Adjust the park brake shoe and lining. Refer to Drum Brake Adjustment in Drum Brakes.

Has the inspection/repair been performed?

--

Go to Step 5

--

5 |

1. Apply the park brake until 4 clicks are heard.
2. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle
3. Use your hands in order to rotate both of the rear wheels forward.

Do either of the rear wheels rotate forward?

--

Go to Step 1

System OK