For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Strut Lower Nuts * | 123 N·m | 90 lb ft
Tie Rod Jam Nuts | 68 N·m | 50 lb ft
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating.

| Refer to the appropriate service procedure for the prevailing torque value.

If the fastener does not meet these criteria, REPLACE the fastener.