For 1990-2009 cars

### Removal Procedure

1. Remove the push-in retainers from the IP insulator to instrument panel.
2. Remove the press-on retainers from the IP insulator to dash mat.
3. Unsnap the IP courtesy lamp from the IP insulator.
4. Remove the IP insulator from the instrument panel.

### Installation Procedure

1. Snap the IP courtesy lamp into the IP insulator.
2. Position the IP insulator to the instrument panel.
3. Install the push-in retainers to the IP insulator to instrument panel.
4. Install the press-on retainers to the IP insulator to dash mat.