For 1990-2009 cars

### Removal Procedure

1. Remove the case side cover pan. Refer to Control Valve Body Cover Replacement .
2. Remove the oil reserve weir.

### Installation Procedure

1. Install the oil reservoir weir.
2. Install the case side cover pan. Refer to Control Valve Body Cover Replacement .
3. Adjust the fluid level.
4. Inspect for the following:

• | Proper completion of repairs

• | Proper fluid level. Refer to Transmission Fluid Check .

• | Fluid leaks. Refer to Fluid Leak Diagnosis and Repair .