For 1990-2009 cars

# LTG REQUEST FOR REVIEW UPDATES 1989 FEB. THRU JUNE 1989

This bulletin addresses changes to the published Pontiac Labor Time Guide, for February through June, 1989 These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future revisions as printed, and at that time it is recommended that you discard the paper copy.

In the case of past model year updates, it is recommended that this bulletin be retained with the appropriate model year labor time guide as a complete revision will not be provided.

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

FINESSE SAND AND BUFF A0110 .3 .3 .3 .3 .3 .3 .3 .3 .3 CB CB CB CB CB CB CB CB CB NOTE: Applicable model year: 1988 ADD: A- For Each Additional Panel .1 .1 .1 .1 .1 .1 .1 .1 .1 CA CA CA CA CA CA CA CA CA

PLENUM AND/OR GASKETS, INTAKE J0130 1.2 - R&R OR REPLACE NOTE: Applicable model years: All w/V-6 ADD: A-To Replace Plenum .4

RUNNERS AND/OR GASKETS, INTAKE - R&R OR REPLA NOTE: Applicable model years: All w/V-6 ONE PIECE J0148 1.8

MANIFOLD AND/OR GASKET, INTAKE J0200 4.6 - REPLACE NOTE: Applicable model years: All w/V-6

COVER AND/OR GASKEL ROCKER - REPLACE NOTE: Applicable model years: All w/V-6 RIGHT BANK J0300 2.0 LEFT BANK J0301 2.3 BOTH BANKS J0307 2.6

ROCKER ARM - REPLACE NOTE: Applicable model years: All w/V-6 ONE CYL RIGHT BANK J0350 2.2 LEFT BANK J0351 2.5 BOTH BANKS J0357 2.9

STUD, ROCKER ARM - REPLACE NOTE: Applicable modeL years: All w/V-6 ONE STUD RIGHT BANK J0380 2.4 LEFT J0381 2.7

GASKET, CYLINDER HEAD - REPLACE NOTE: Applicable model years: All w/V-6 RIGHT BANK J0500 6.1 LEFT BANK J0501 6.3 BOTH BANKS J0507 7.4

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

HEAD, CYLINDER - REPLACE NOTE: Applicable model years: All w/V-6 RIGHT BANK J0510 7.0 LEFT BANK J0511 7.1 BOTH BANKS J0517 9.0

VALVE - RECONDITION OR REPLACE NOTE: Applicable model years: All w/ V-6 ONE CYL RIGHT BANK J0520 6.7 LEFT BANK J0521 6.9 BOTH BANKS J0527 8.6

SPRING, CAP AND/OR SEAL, VALVE - REPLACE NOTE: Applicable model years: All w/V-6 ONE CYL RIGHT BANK J0540 2.5 LEFT BANK J0541 2.8 BOTH BANKS J0547 3.4

PUSH ROD - REPLACE NOTE: Applicable model years: All w/V-6 ONE CYL RIGHT BANK J0580 2.2 LEFT BANK J0581 2.5 BOTH BANKS J0587 2.9

LIFTER, VALVE - REPLACE NOTE: Applicable model years: All w/V-6 ONE CYL RIGHT BANK J0620 4.8 LEFT BANK J0621 4.8 BOTH BANKS J0627 5.0

PAN AND/OR GASKET, OIL J1000 2.7 - REPLACE NOTE: Applicable model years: All w/V-6

PUMP, ENGINE OIL-REPLACE J1020 2.8 NOTE: Applicable model years: All w/ V-6

BEARING, CRANKSHAFT MAIN - REPLACE 3.3 NOTE: Applicable model years: All w/ V-6

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

BEARING, CONNECTING ROD - REPLACE 3.3 NOTE: Applicable model years: All w/V-6

CRANKSHAFT-REPLACE J1200 10.1 NOTE: Applicable model years: 1984-87 w/L-4 ADD: A- With A/C 1.0

PISTON, ROD AND/OR RINGS - REPLACE NOTE: Applicable model years: All w/V-6 ONE CYL RIGHT BANK J1300 9.1 LEFT BANK J1301 9.3 BOTH BANKS J1307 11.0

PUMP AND/OR GASKET, COOLANT J3480 1.9 - REPLACE NOTE: Applicable model years: 1987-88 w/L-4 ADD: A- With A/C .1

PICK-UP COIL AND/OR POLE PIECE, DISTRIBUTOR - REPLACE J4460 1.3 NOTE: Applicable model year: 1985 w/ V-6

INJECTOR, FUEL-REPLACE J5650 1.9 NOTE: Applicable model years: All w/V-6

RAIL, FUEL - REPLACE J5660 1.7 NOTE: Applicable model years: All w/V-6

SENSOR, MASS AIR FLOW-REPLACE J5670 .6 NOTE: Applicable model years: All w/V-6

ELECTRONICALLY CONTROLLED EMISSIONS AND FUEL SYSTEM - REPLACE NOTE: Applicable model years: 1986-87 W/3.8L IDLE SPEED CONTROL MOTOR J6410 .5 ADD: A- To Perform C.C.C. System Performance Check .5

TACHOMETER - R&R N4500 .9 NOTE: Applicable model years: 1984-86

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

TACHOMETER - REPLACE N4510 .9 NOTE: Applicable model years: 1984-86

CAMPAIGN 84-C-15B NOTE: Applicable model year: 1984 w/L-4 WITHOUT A/C V4388 12.7 WITH A/C V4389 13.7

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

FINESSE SAND AND BUFF A0110 .3 .3 .3 .3 .3 .3 .3 .3 .3 CB CB CB CB CB CB CB CB CB NOTE: Applicable model years: 1988-89 ADD: A- For Each Additional Panel .1 .1 .1 .1 .1 .1 .1 .1 .1 CA CA CA CA CA CA CA CA CA

SEAL, FRONT DOOR JAMB SWITCH - REPLACE NOTE: Applicable model years: 1988-89 RIGHT B4110 .2 .2 .2 .2 .2 .2 .2 LEFT B4111 .2 .2 .2 .2 .2 .2 .2

SEAL, REAR DOOR JAMB SWITCH - REPLACE NOTE: Applicable model years: 1988-89 RIGHT B4510 .2 .2 .2 .2 .2 .2 .2 LEFT B4511 .2 .2 .2 .2 .2 .2 .2

COVER, HIGH LEVEL STOP LAMP B5650 .3 - REPLACE NOTE: Applicable model years: 1988-89 ADD: A- To Color Coat .2 CA MOLDING, REAR DOOR - R&R OR REPLACE NOTE: Applicable model years: 1988-89 RIGHT SIDE B7966 .5 LEFT SIDE B7976 .5

MOLDING, BACK WINDOW REVEAL B8520 .4 - R&R OR REPLACE NOTE: Applicable model years: 1988-89

TAPE AND/OR GUIDE BLOCK, FRONT DOOR WINDOW REGULATOR - REPLACE NOTE: Applicable model years: 1989-90 RIGHT C0174 .7 LEFT C0175 .7

CARPET, FLOOR - R&R OR REPLACE NOTE: Applicable model years: 1988-90 ONE PIECE C4208 1.4 ADD: A- W/Console .7

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

CABLES, AIR DISTRIBUTION - R&R OR REPLACE NOTE: Applicable model years: 1988-89 AIR CONDITIONING D0447 .9 TEMPERATURE

MOTOR AND/OR FAN, BLOWER-R&R OR REPLACE NOTE:Applicable model year: 1987 A/C D1322 .8

SHIELD, DISC BRAKE SPLASH - R&R OR REPLACE NOTE: Applicable model year: 1988 FRONT RIGHT H0160 .3 LEFT H0161 .3 BOTH H0167 .4 REAR RIGHT H0170 .3 LEFT H0171 .3 BOTH H0177 .5

SENSOR, FLUID LEVEL-REPLACE H2493 .2 NOTE: Applicable model years: 1987-88

GASKET, CYLINDER HEAD-REPLACE J0508 6.7 6.7 NOTE: Applicable model years: 1987-89 W/OHC-4 ADD: A- With A/C .2 .2 B- With P/S 1.3 1.3 C- W/Turbocharger 1.2 1.2

HEAD, CYLINDER - REPLACE J0518 8.1 8.1 NOTE: Applicable model years: 1987-89 w/OHC-4 ADD: A- With A/C .2 .2 B- With P/S 1.3 1.3 C- W/Turbocharger 1.2 1.2

VALVE - RECONDITION OR REPLACE J0528 7.2 7.2 NOTE: Applicable model years: 1987-89 w/OHC-4 ADD: A- With A/C .2 .2 B- With P/S 1.3 1.3 C- W/Turbocharger 1.2 1.2

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION A B F H J N T U W OPERATION DESCRIPTION NUMBER VIN CODE

CAMSHAFT - REPLACE J0850 3.8 3.8 NOTE: Applicable model years 1982-89 w/ OHC-4 ADD: A-With A/C .2 .2 B-With P/S .3 .3

SUPPORT, CAMSHAFT - REPLACE J0860 6.7 6.7 NOTE: Applicable model years: 1987-89 w/ OHC-4 ADD: A-With A/C .2 .2 B-With P/S 1.3 1.3 C- W/Turbocharger 1.2 1.2

GASKET,CYLINDER HEAD-REPLACE J0508 7.8 NOTE: Applicable model yeaRS: 1988-89 w/ Quad 4

VALVE, OIL FLOW CHECK-REPLACE J0509 7.9 NOTE: Applicable model years:1988-89 W/ Quad 4 ADD: A-To Clean Parts On Vehicles Over 30,000 Miles If Nec .4

PUMP, ENGINE OIL - REPLACE J1020 1.7 NOTE: Applicable model years: 1988-89 w/Quad 4

DRIVE, OIL PUMP - REPLACE J1050 .8 .8 NOTE: Applicable model years: 1987-89 w/ V-6

PAN AND/OR GASKET, OIL-REPLACE J1000 1.6 NOTE: Applicable model years: 1988-89 w/ V-8 ADD: A- With A/C .3

ENGINE, PARTIAL/BASIC-REPLACE J1820 11.8 NOTE: Applicable model years: 1987-89 V-8 w/ port injection ADD: A-With A/C .5

SENSOR, COOLANT LEVEL - REPLACE J3032 .3 NOTE: Applicable model year: 1989

HOSE, ENGINE COOLANT - REPLACE NOTE: Applicable model years: 1987-89 w/ Engine Code K INTAKE MANIFOLD J3365 1.2

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

PUMP AND/OR GASKET, COOLANT J3480 -REPLACE NOTE: Applicable model years: 1989 OHC-4; 1985-88 L-4 OHC-4 2.7 2.7 L-4 1.5 ADD: A-With A/C (OHC-4) .2 .2

INTEGRATED DIRECT IGNITION SYSTEM COMPONENTS - REPLACE NOTE: Applicable model year: 1988 w/ Quad 4 COIL J4405 POLICY: E MODULE J4410 POLICY: E

JETS, MAIN METERING-REPLACE J5090 .9 NOTE: Applicable model years: 1985-86 w/ V-8 ADD: A- To Perform C.C.C. System Performance .5 Check

BODY, THROTTLE - R&R J5485 1.1 NOTE: Applicable model years: 1987-88 w/ V-6

BODY UNIT, THROTTLE-REPLACE J5490 1.1 NOTE: Applicable model years: 1987-88 w/ V-6

TRANSAXLE ASSEMBLY - REPLACE K7000 4.6 NOTE: Applicable model year: 1988

CONVERTER ASSEMBLY, TRANSAXLE K7020 3.6 - REPLACE NOTE: Applicable model year: 1988

SEAL, TRANSAXLE CONVERTER K7060 3.0 - REPLACE NOTE: Applicable model year: 1988

DIRECT CLUTCH, FORWARD CLUTCH, INTERMEDIATE BAND - REPLACE K7200 4.2 NOTE: Applicable model year: 1988

COVER AND/OR GASKETS, TRANSAXLE K7500 4.1 CASE - REPLACE NOTE: Applicable model year: 1988

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

LINK ASSEMBLY, TRANSAXLE DRIVE K7520 4.1 - REPLACE NOTE: Applicable model year: 1988

PARKING LOCK ACTUATOR, MANUAL SHAFT AND/OR LEVER AND HUB ASSEMBLIES - REPLACE K7540 4.2 NOTE: Applicable model year: 1988

INPUT INTERNAL GEAR, CARRIER ASSEMBLY, INPUT SUN GEAR AND INPUT DRUM-REPLACE K7560 4.6 NOTE: Applicable model year: 1988

CLUTCH,LOW AND REVERSE-REPLACE K7580 4.4 NOTE: Applicable model year: 1988

REACTION GEAR SET, TRANSAXLE K7600 4.5 - REPLACE NOTE: Applicable model year: 1988

DIFFERENTIAL AND FINAL DRIVE ASSEMBLY, TRANSAXLE - REPLACE K7620 4.6 NOTE: Applicable model year: 1988

DRIVE GEAR, TRANSAXLE GOVERNOR K7680 4.8 - REPLACE NOTE: Applicable model year: 1988

CASE, TRANSAXLE - REPLACE K7800 4.6 NOTE: Applicable model year: 1988

MOUNT AND/OR BRACKET, TRANSAXLE - REPLACE NOTE: Applicable model years: 1986-88 w/ V-6 FRONT K6722 .5 REAR K6723 1.2 BOTH K6727 1.4

CABLES, BATTERY - REPLACE NOTE: Applicable model years: 1987-89 NEGATIVE ONE N0126 .3

#### REQUEST FOR REVIEW

OPERATION DESCRIPTION OPERATION VEHICLE SERIES NUMBER A B F H J N T U W VIN CODE

SEALED BEAM AND/OR RETAINING RING, HEADLAMP - REPLACE NOTE: Applicable model years: 1987-89 RIGHT N0300 .3 LEFT N0301 .3

BULBS, LAMP - REPLACE INSTRUMENT PANEL CLUSTER N0627 .6 (ONE OR ALL) NOTE: Applicable model years: 1987-89

INSTRUMENT PANEL WARNING N0647 .6 (ONE OR ALL) NOTE: Applicable model years: 1987-89 SIDE MARKER REAR (ONE OR BOTH) N0747 .4 NOTE: Applicable model years: 1987-89

LENS AND/OR GASKET, LAMP - REPLACE SIDE MARKER FRONT (ONE OR BOTH) N1257 .3 NOTE: Applicable model years: 1988-89 SIDE MARKER REAR (ONE OR BOTH) N1267 .5 NOTE: Applicable model years: 1988-89 STOP, TAIL AND TURN SIGNAL ALL N1287 .7 NOTE: Applicable model years: 1988-89

LAMP ASSEMBLY-REPLACE SIDE MARKER RIGHT FRONT N1564 .3 NOTE: Applicable model years: 1988-89 SIDE MARKER LEFT FRONT N1565 .3 NOTE: Applicable model years: 1988-89 SIDE MARKER RIGHT REAR N1574 .3 NOTE: Applicable model years: 1988-89 SIDE MARKER LEFT REAR N1575 .3 NOTE: Applicable model years: 1988-89 STOP,CENTER HIGH LEVEL N1600 .3 NOTE: Applicable model years: 1988-89

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

SWITCH - REPLACE DOOR WINDOW RIGHT FRONT N2144 .4 NOTE: Applicable model years: 1988-89 DOOR WINDOW LEFT FRONT N2145 .4 NOTE: Applicable model years: 1988-89 DOOR JAMB RIGHT FRONT N2174 .3 NOTE: Applicable model years: 1988-89 DOOR JAMB LEFT FRONT N2175 .3 NOTE: Applicable model years: 1988-89 ENGINE OIL PRESSURE N2220 .3 NOTE: Applicable model years: 1988-89 ENGINE COOLANT TEMPERATURE N2230 .5 NOTE: Applicable model years: 1988-89 HEADLAMP N2290 .6 NOTE: Applicable model years: 1988-89 INSTRUMENT PANEL DIMMER N2317 .6 AND INTERIOR LAMP ON/OFF NOTE: Applicable model years: 1988-89 IGNITION N2320 .7 NOTE: Applicable model years: 1988-89 KEY WARNING N2330 .9 NOTE: Applicable model years: 1988-89 MAP/READING N2350 .3 NOTE: Applicable model years: 1988-89 CLUTCH START N2360 .5 NOTE: Applicable model years: 1988-89 FRONT COMPARTMENT LID AJAR N2382 .2 NOTE: Applicable model year: 1989 SEAT ADJUSTER LEFT N2411 .3 NOTE: Applicable model years: 1987-89 SEAT LUMBAR CONTROL ADJUST RIGHT N2416 .3 NOTE: Applicable model years: 1988-89

SWITCH - REPLACE SEAT LUMBAR CONTROL ADJUST LEFT N2417 .3 NOTE: Applicable model years: 1988-89 SEAT AIR DIRECTIONAL N2418 .4 CONTROL ADJUST NOTE: Applicable model year: 1989 WIPER WINDSHIELD N2610 1.1 NOTE: Applicable model years: 1988-89

RELAY - REPLACE ENGINE COOLANT FAN N2850 .3 NOTE: Applicable model years: 1988-89 FOG LAMP N2856 .3 NOTE: Applicable model years: 1988-89

CONTACT, ELECTRICAL - REPLACE HATCH BODY SIDE N3020 .2 NOTE: Applicable model years: 1988-89

ACTUATOR ASSEMBLY - REPLACE HEADLAMP RIGHT N3230 .6 NOTE: Applicable model years: 1988-89 HEADLAMP LEFT N3231 .6 NOTE: Applicable model years: 1988-89 REAR COMPARTMENT LID RELEASE N3270 .4 NOTE: Applicable model years: 1987-89

HEADLAMP WASHER SYSTEM COMPONENTS - REPLACE WASHER FLUID CONTAINER N3671 .6 NOTE: Applicable model years: 1988-89

HEAD, SPEEDOMETER - R&R N4300 .6 NOTE: Applicable model years: 1988-89

HEAD, SPEEDOMETER - REPLACE N4310 .6 NOTE: Applicable model years: 1988-89

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

GAGE - REPLACE FUEL (DASH UNIT) N4680 .7 NOTE: Applicable model years: 1988-89

RADIO RECEIVER - R&R R0750 .7 NOTE: Applicable model year: 1989

SPEAKER, RADIO - REPLACE NOTE: Applicable model years: 1988-90 REAR RIGHT R0950 .4 LEFT R0951 .4

MODULE, CRUISE CONTROL R1220 .5 - REPLACE NOTE: Applicable model years: 1988-89

MIRROR, OUTSIDE REAR VIEW - REPLACE NOTE: Applicable model years: 1988-89 MANUAL RIGHT R3260 .6 LEFT R3261 .6 REMOTE CONTROL RIGHT R3280 .7 LEFT R3281 .7

HANDLE, FUEL FILLER DOOR LOCK R4080 .3 RELEASE - REPLACE NOTE: Applicable model years: 1988-89

RECEIVER, REMOTE DOOR/REAR R4480 .8 COMPARTMENT LOCK REPLACE NOTE: Applicable model year: 1989

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.