For 1990-2009 cars

### Removal Procedure

The fuel pump relay (1) is mounted in the right front corner of the engine compartment.

1. Turn the ignition OFF.
2. Remove the negative battery cable.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

3. Remove the under hood electrical center cover.
4. Remove the fuel pump relay from the under hood electrical center.

### Installation Procedure

1. Install the fuel pump relay (1) into the under hood electrical center.
2. Install the under hood electrical center cover.
3. Install the negative battery cable.
4. Turn the ignition ON.