For 1990-2009 cars

### Removal Procedure

1. Use a small, flat-bladed tool in order to release the retainers and remove the dome lamp from the headliner.
2. Disconnect the electrical connectors from the dome lamp.
3. Remove the dome lamp from the headliner.
4. Use a small, flat-bladed tool in order to remove the dome lamp lens from the dome lamp.
5. Use a small, flat-bladed tool in order to remove the bulb from the socket.

### Installation Procedure

1. Press the bulb into the socket.
2. Snap the dome lamp lens into the dome lamp.
3. Connect the electrical connectors to the dome lamp.
4. Install the dome lamp to the headliner.
5. Press the dome lamp into the hole in the headliner in order to snap-in the retainers.